



**Smart Door&Window Sensor**

***Premium Add-on device for your home***

This is smart door/window sensor, adopts super low power consumption ZigBee wireless networking technology, makes a longer battery life-span, can feel open or close state of the door or window through closing and seperating between sensor and magnetic, dual sensor design, flexible and adaptable, products are suitable for home, villa, factories, shops, banks, office building and other place of safety prevention.

Specification

* Model Number: HS1DS-TY
* Working Voltage: DC3V
* Battery Type: 2xAAA battery
* Battery Life: 2 years
* Standby Current: <10 uA
* Alarm Current: ≤36mA
* Install Height: surface mounted
* Networking Way: ZigBee 2.4GHz
* Sensitivity: 15m
* Anti-RF Interference: 80MHz — 1GHz 10V/m
* Operating Environment: -10℃ ～ +50℃
* Working Humidity: ≤95%RH
* Transmitter Dimensions: 76x36.6x16.5 mm
* Magnet Dimensions: 76x13.9x16.5mm
* Gross Weight: 67g

***Features***

* **Standard ZigBee protocol, good compatibility;**
* **Super low power consumption design, battery lifespan up to 24 months;**
* **Real time monitoring closed/open start of door or window;**
* **Double reed switch design, suitable for door or window with different direction;**
* **Support anti-dismantle alarm;**
* **Easy replacement of the battery;**
* **Low power alert and report function;**
* **Free tool installation, stick and play;**
* **Smart and fasion design, with appearance design patent;**
* **CE, ROHS, FCC approval**